Size of smallest allocations in RIPE NCC CIDR blocks

Size of smallest allocations in CIDR blocks allocated by the RIPE NCC

JoŸao Luis Silva Damas

RIPE NCC

Document: ripe 211 Date: July 26, 2000

Size of smallest allocations in RIPE NCC CIDR blocks

This document contains the size of the minimum and default allocations made by the RIPE NCC to users from CIDR blocks assigned to the RIPE NCC by the IANA.

ŞDefault allocationŤ refers to the amount of addresses, in pre^x notation, that are allocated to users by default.

ŞSmallest allocationŤ refers to the size of the smallest allocation, in pre^x notation, made by the RIPE NCC to a user.

Allocations smaller than the default size have been made to users requesting Provider Independent (PI) address space.

Routing decisions for blocks of address space are the sole responsibility of network operators.

However, network operators taking routing decisions based on pre^x length are requested and encouraged to route at least blocks of sizes corresponding to the Şdefault allocationŤ and bigger.

Users to whom small blocks (smaller than the default allocation size) of PI addresses are given out are always noti^ed that network operators throughout the Internet may choose not to route, or may ^lter, small address blocks if they are not aggregated into bigger blocks. This is, as a matter of fact, common practice nowadays.

CIDR block Default allocation Smallest allocation 62/8 /19 /19 193/8 /19 /29 194/8 /19 /29 195/8 /19 /29 212/8 /19 /19 213/8 /19 /19 217/8 /20 NA

Table 1. Allocation sizes for CIDR blocks from which the RIPE NCC has made allocations.